Return to contents

LocalRemoteControlState A value representing the current state of control associated with the device. Examples: A device can either work autonomously (localRemoteControlStateCode="Local") or it can be controlled by another system (localRemoteControlStateCode="Remote"). Rationale: The control status of a device must be communicated between devices prior to remote commands being transmitted. If the device is not in "Remote" status then external commands will be ignored.
Lvl | Type, Domain name and/or Mnemonic code | Concept ID | Mnemonic | Print Name | Definition/Description
--- | --- | --- | --- | --- | ---
1 | L: (L) | C10894 | L | Local | An equipment can either work autonomously ('Local' control state).
1 | L: (R) | C10895 | R | Remote | An equipment can be controlled by another system, e.g., LAS computer ('Remote' control state).

Return to contents

Last Published: 03/27/2006 3:35 AM

HL7® Version 3 Standard, © 2005 Health Level Seven®, Inc. All Rights Reserved.

HL7 and Health Level Seven are registered trademarks of Health Level Seven, Inc. Reg. U.S. Pat & TM Off