Return to contents

CommunicationFunctionType Describes the type of communication function that the associated entity plays in the associated transmission.
Lvl | Type, Domain name and/or Mnemonic code | Concept ID | Mnemonic | Print Name | Definition/Description
--- | --- | --- | --- | --- | ---
1 | L: (RCV) | C16033 | RCV | receiver | The entity is the receiver of the transmission.
1 | L: (RSP) | C16034 | RSP | respond to | The entity is the one to which the response or reply to the transmission should be sent.
1 | L: (SND) | C16032 | SND | sender | The entity is the sender of the transmission.

Return to contents

Last Published: 03/27/2006 3:35 AM

HL7® Version 3 Standard, © 2005 Health Level Seven®, Inc. All Rights Reserved.

HL7 and Health Level Seven are registered trademarks of Health Level Seven, Inc. Reg. U.S. Pat & TM Off