Return to contents

ResponseMode Specifies the mode, immediate versus deferred or queued, by which a receiver should communicate its receiver responsibilities.
Lvl | Type, Domain name and/or Mnemonic code | Concept ID | Mnemonic | Print Name | Definition/Description
--- | --- | --- | --- | --- | ---
1 | L: (D) | C21433 | D | deferred | The receiver may respond in a non-immediate manner. Note: this will be the default value.
1 | L: (I) | C21432 | I | immediate | The receiver is required to assume that the sender is blocking and behave appropriately by sending an immediate response.
1 | L: (Q) | C21434 | Q | queue | The receiver shall keep any application responses in a queue until such time as the queue is polled.

Return to contents

Last Published: 03/27/2006 3:35 AM

HL7® Version 3 Standard, © 2005 Health Level Seven®, Inc. All Rights Reserved.

HL7 and Health Level Seven are registered trademarks of Health Level Seven, Inc. Reg. U.S. Pat & TM Off