Return to contents

ProcessingMode This attribute defines whether the message is being sent in current processing, archive mode, initial load mode, restore from archive mode, etc.
Lvl | Type, Domain name and/or Mnemonic code | Concept ID | Mnemonic | Print Name | Definition/Description
--- | --- | --- | --- | --- | ---
1 | L: (A) | C10121 | A | Archive | Identifies archive mode of processing.
1 | L: (T) | C10124 | T | Current processing | Identifies on-line mode of processing.
1 | L: (I) | C10123 | I | Initial load | Identifies initial load mode of processing.
1 | L: (R) | C10122 | R | Restore from archive | Identifies restore mode of processing.

Return to contents

Last Published: 03/27/2006 3:35 AM

HL7® Version 3 Standard, © 2005 Health Level Seven®, Inc. All Rights Reserved.

HL7 and Health Level Seven are registered trademarks of Health Level Seven, Inc. Reg. U.S. Pat & TM Off