Return to contents

AcknowledgementDetailCode A site specific problem code
Lvl | Type, Domain name and/or Mnemonic code | Concept ID | Mnemonic | Print Name | Definition/Description
--- | --- | --- | --- | --- | ---
1 | A: AcknowledgementDetailNotSupportedCode | A19640 |  |  | Refelects rejections because elements of the communication are not supported in the current context.
2 | L: (NS260) | C21424 | NS260 | Unknown sender | The Device.id of the sender is unknown.
2 | L: (NS261) | C21425 | NS261 | Unrecognized attentionline | The receiver requires information in the attentionLine classes for routing purposes.
2 | L: (NS200) | C21420 | NS200 | Unsupported interaction | The interaction (or: this version of the interaction) is not supported.
2 | L: (NS250) | C21422 | NS250 | Unsupported processing Mode | The processing mode is not supported.
2 | L: (NS202) | C21421 | NS202 | Unsupported processing id | The Processing ID is not supported.
2 | L: (NS203) | C21423 | NS203 | Unsupported version id | The Version ID is not supported.
1 | A: AcknowledgementDetailSyntaxErrorCode | A19639 |  |  | Reflects errors in the syntax or structure of the communication.
2 | L: (SYN102) | C21414 | SYN102 | Data type error | The attribute contained data of the wrong data type, e.g. a numeric attribute contained "FOO".
2 | L: (SYN104) | C21416 | SYN104 | Invalid code system in CNE | An attribute value referenced a code system that is not valid for an attribute constrained to CNE.
2 | L: (SYN110) | C21417 | SYN110 | Number of association repetitions exceeds limit | The number of repetitions of a (group of) association(s) exceeds the limits of the standard or of one of the conformance profiles identified in the message.
2 | L: (SYN112) | C21418 | SYN112 | Number of attribute repetitions exceeds limit | The number of repetitions of an attribute exceeds the limits of the standard or of one of the conformance profiles identified in the message.
2 | L: (SYN100) | C21412 | SYN100 | Required association missing | Required association missing in message; or the sequence of the classes is different than required by the standard or one of the conformance profiles identified in the message.
2 | L: (SYN101) | C21413 | SYN101 | Required attribute missing | A required attribute is missing in a class.
2 | L: (SYN103) | C21415 | SYN103 | Value not found in code system | An attribute value was compared against the corresponding code system, and no match was found.
1 | L: (RTUDEST) | C21440 | RTUDEST | Error: Message routing error, unknown destination. | The destination of this message is unknown to the receiving application. The receiving application in the message does not match the application which received the message. The message was neither routed, processed nor stored by the receiving application.
1 | L: (RTEDEST) | C21443 | RTEDEST | Message routing error, destination unreachable. | Error: The destination of this message is known to the receiving application. Messages have been successfully routed to that destination in the past. The link to the destination application or an intermediate application is unavailable.
1 | L: (RTWDEST) | C21441 | RTWDEST | Message routing warning, destination unreachable. | Warning: The destination of this message is known to the receiving application. Messages have been successfully routed to that destination in the past. The link to the destination application or an intermediate application is (temporarily) unavailable. The receiving application will forward the message as soon as the destination can be reached again.
1 | L: (NOSTORE) | C21442 | NOSTORE | No storage space for message. | Rejection: The message can't be stored by the receiver due to an unspecified internal application issue. The message was neither processed nor stored by the receiving application.

Return to contents

Last Published: 03/27/2006 3:35 AM

HL7® Version 3 Standard, © 2005 Health Level Seven®, Inc. All Rights Reserved.

HL7 and Health Level Seven are registered trademarks of Health Level Seven, Inc. Reg. U.S. Pat & TM Off